Filetype: IR signals file
Version: 1
# 
# Manta TV
#
name: On
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 00 FF 00 00
# 
name: VOL+
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 48 B7 00 00
# 
name: VOL-
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 49 B6 00 00
# 
name: CH+
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 4A B5 00 00
# 
name: CH-
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 4B B4 00 00
# 
name: MUTE
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 01 FE 00 00
# 
name: Source
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 16 E9 00 00
# 
name: Ok
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 10 EF 00 00
# 
name: Up
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 13 EC 00 00
# 
name: Down
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 14 EB 00 00
# 
name: Left
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 11 EE 00 00
# 
name: Right
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 12 ED 00 00
# 
name: Aspect
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 64 9B 00 00
# 
name: Menu
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 40 BF 00 00
# 
name: Exit
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 15 EA 00 00
