Filetype: IR signals file
Version: 1
# 
# Samsung SC18M31A0HU Vacuum
#
name: POWER
type: parsed
protocol: NEC
address: 21 00 00 00
command: 0B 00 00 00
# 
name: Min/Mid
type: parsed
protocol: NEC
address: 21 00 00 00
command: 08 00 00 00
# 
name: Max
type: parsed
protocol: NEC
address: 21 00 00 00
command: 01 00 00 00
