Filetype: IR signals file
Version: 1
#
name: EXIT
type: parsed
protocol: NECext
address: 00 99 00 00
command: 02 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 00 99 00 00
command: 08 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 99 00 00
command: 09 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 99 00 00
command: 0C 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 99 00 00
command: 0D 00 00 00
#
name: SCAN_<<
type: parsed
protocol: NECext
address: 00 99 00 00
command: 0E 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 99 00 00
command: 0F 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 99 00 00
command: 11 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 00 99 00 00
command: 12 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 99 00 00
command: 13 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 00 99 00 00
command: 14 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 99 00 00
command: 15 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 99 00 00
command: 17 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 99 00 00
command: 19 00 00 00
#
name: SCAN_>>
type: parsed
protocol: NECext
address: 00 99 00 00
command: 1A 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 99 00 00
command: 1B 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 99 00 00
command: 1D 00 00 00
#
name: SKIP_<<
type: parsed
protocol: NECext
address: 00 99 00 00
command: 1E 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 99 00 00
command: 1F 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 00 99 00 00
command: 4D 00 00 00
#
name: SKIP_>>
type: parsed
protocol: NECext
address: 00 99 00 00
command: 5B 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 00 99 00 00
command: 5C 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 00 99 00 00
command: 5D 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: 00 99 00 00
command: 5E 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: 00 99 00 00
command: 5F 00 00 00
