Filetype: IR signals file
Version: 1
#
name: 1_MUTE/UNMUTE_80_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 01 00 00 00
#
name: 5_VOL_-_40_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 02 00 00 00
#
name: 4_VOL_+_C0_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 03 00 00 00
#
name: 7_AM_30_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 0C 00 00 00
#
name: 12_VIDEO_2_B0_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 0D 00 00 00
#
name: 11_VIDEO_1_70_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 0E 00 00 00
#
name: 13_AUX_F0_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 0F 00 00 00
#
name: 8_FM_08_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 10 00 00 00
#
name: 23_SKIP_REV_18_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 18 00 00 00
#
name: 24_SKIP_FWD_98_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 19 00 00 00
#
name: 25_STOP_58_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 1A 00 00 00
#
name: 26_AM/FM_PRESET_+_B8
type: parsed
protocol: NECext
address: BA 85 00 00
command: 1D 00 00 00
#
name: 27_AM/FM_PRESET_-_F8
type: parsed
protocol: NECext
address: BA 85 00 00
command: 1F 00 00 00
#
name: 29_RANDOM_DISK_52_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 4A 00 00 00
#
name: 14_OFF_32_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 4C 00 00 00
#
name: 15_TAPE_4A_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 52 00 00 00
#
name: 16_CD_CA_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 53 00 00 00
#
name: 28_DISK_-_2A_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 54 00 00 00
#
name: 19_PLAY_AA_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 55 00 00 00
#
name: 18_PAUSE_6A_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 56 00 00 00
#
name: 20_FAST_REV_EA_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 57 00 00 00
#
name: 21_FAST_FWD_1A_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 58 00 00 00
#
name: 22_RANDOM_3A_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 5C 00 00 00
#
name: 17_NEXT_DISK_BA_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: 5D 00 00 00
#
name: 30_MUTE_ALL_FB_A1
type: parsed
protocol: NECext
address: BA 85 00 00
command: DF 00 00 00
