Filetype: IR signals file
Version: 1
#
# TELESYSTEM TS3002
# Autogenerated from ircodes/TELESYSTEM/TS3002.xml
#
name: POWER
type: parsed
protocol: NECext
address: 5F 80 00 00
command: B7 48 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 5F 80 00 00
command: F7 08 00 00
#
name: TV/SAT
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 97 68 00 00
#
name: 1
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 7F 80 00 00
#
name: 2
type: parsed
protocol: NECext
address: 5F 80 00 00
command: BF 40 00 00
#
name: 3
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 3F C0 00 00
#
name: 4
type: parsed
protocol: NECext
address: 5F 80 00 00
command: DF 20 00 00
#
name: 5
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 5F A0 00 00
#
name: 6
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 9F 60 00 00
#
name: 7
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 1F E0 00 00
#
name: 8
type: parsed
protocol: NECext
address: 5F 80 00 00
command: EF 10 00 00
#
name: 9
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 6F 90 00 00
#
name: Guide
type: parsed
protocol: NECext
address: 5F 80 00 00
command: BD 42 00 00
#
name: 0
type: parsed
protocol: NECext
address: 5F 80 00 00
command: FF 00 00 00
#
name: FAV
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 7D 82 00 00
#
name: Audio
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 9D 62 00 00
#
name: CH
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 27 D8 00 00
#
name: Video
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 95 6A 00 00
#
name: VOL
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 87 78 00 00
#
name: OK
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 25 DA 00 00
#
name: VOL
type: parsed
protocol: NECext
address: 5F 80 00 00
command: A7 58 00 00
#
name: Menu
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 37 C8 00 00
#
name: CH
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 07 F8 00 00
#
name: Exit
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 57 A8 00 00
#
name: Text
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 77 88 00 00
#
name: Display
type: parsed
protocol: NECext
address: 5F 80 00 00
command: A5 5A 00 00
#
name: Back
type: parsed
protocol: NECext
address: 5F 80 00 00
command: FD 02 00 00
#
name: Epg
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 6D 92 00 00
#
name: Opt?
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 8D 72 00 00
#
name: App
type: parsed
protocol: NECext
address: 5F 80 00 00
command: ED 12 00 00
#
name: Info
type: parsed
protocol: NECext
address: 5F 80 00 00
command: D7 28 00 00
#
name: R
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 4D B2 00 00
#
name: G
type: parsed
protocol: NECext
address: 5F 80 00 00
command: 2D D2 00 00
#
name: Y
type: parsed
protocol: NECext
address: 5F 80 00 00
command: E7 18 00 00
#
name: B
type: parsed
protocol: NECext
address: 5F 80 00 00
command: AD 52 00 00
