Filetype: IR signals file
Version: 1
# 
name: On_off
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 02 00 00 00
# 
name: Up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: Down
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 61 00 00 00
# 
name: Left
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 65 00 00 00
# 
name: Right
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 62 00 00 00
# 
name: Back
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 58 00 00 00
# 
name: VOL+
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 07 00 00 00
# 
name: VOL-
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0B 00 00 00
# 
name: Hdmi
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 01 00 00 00
# 
name: Ok
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 68 00 00 00
# 
name: MUTE
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0F 00 00 00
# 
name: Home
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 79 00 00 00
