Filetype: IR signals file
Version: 1
# 
# LG magic remote for the LG C9
# receiver POWER, voice control, scrolling and gyro do not use IR, and so are not in this file
# 
name: POWER
type: parsed
protocol: NEC
address: 04 00 00 00
command: 08 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: 04 00 00 00
command: 11 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: 04 00 00 00
command: 12 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: 04 00 00 00
command: 13 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: 04 00 00 00
command: 14 00 00 00
# 
name: 5
type: parsed
protocol: NEC
address: 04 00 00 00
command: 15 00 00 00
# 
name: 6
type: parsed
protocol: NEC
address: 04 00 00 00
command: 16 00 00 00
# 
name: 7
type: parsed
protocol: NEC
address: 04 00 00 00
command: 17 00 00 00
# 
name: 8
type: parsed
protocol: NEC
address: 04 00 00 00
command: 18 00 00 00
# 
name: 9
type: parsed
protocol: NEC
address: 04 00 00 00
command: 19 00 00 00
# 
name: List
type: parsed
protocol: NEC
address: 04 00 00 00
command: 4C 00 00 00
# 
name: 0
type: parsed
protocol: NEC
address: 04 00 00 00
command: 10 00 00 00
# 
name: VOL+
type: parsed
protocol: NEC
address: 04 00 00 00
command: 02 00 00 00
# 
name: VOL-
type: parsed
protocol: NEC
address: 04 00 00 00
command: 03 00 00 00
# 
name: MUTE
type: parsed
protocol: NEC
address: 04 00 00 00
command: 09 00 00 00
# 
name: CH+
type: parsed
protocol: NEC
address: 04 00 00 00
command: 00 00 00 00
# 
name: CH-
type: parsed
protocol: NEC
address: 04 00 00 00
command: 01 00 00 00
# 
name: Home
type: parsed
protocol: NEC
address: 04 00 00 00
command: 7C 00 00 00
# 
name: Settings
type: parsed
protocol: NEC
address: 04 00 00 00
command: 43 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: 04 00 00 00
command: 40 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: 04 00 00 00
command: 07 00 00 00
# 
name: Enter
type: parsed
protocol: NEC
address: 04 00 00 00
command: 44 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: 04 00 00 00
command: 06 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: 04 00 00 00
command: 41 00 00 00
# 
name: Back
type: parsed
protocol: NEC
address: 04 00 00 00
command: 28 00 00 00
# 
name: Guide
type: parsed
protocol: NEC
address: 04 00 00 00
command: AB 00 00 00
# 
name: Netflix
type: parsed
protocol: NEC
address: 04 00 00 00
command: 56 00 00 00
# 
name: Inputs
type: parsed
protocol: NEC
address: 04 00 00 00
command: 0B 00 00 00
# 
name: Prime_video
type: parsed
protocol: NEC
address: 04 00 00 00
command: 5C 00 00 00
# 
name: Red
type: parsed
protocol: NEC
address: 04 00 00 00
command: 72 00 00 00
# 
name: Green
type: parsed
protocol: NEC
address: 04 00 00 00
command: 71 00 00 00
# 
name: Yellow
type: parsed
protocol: NEC
address: 04 00 00 00
command: 63 00 00 00
# 
name: Blue
type: parsed
protocol: NEC
address: 04 00 00 00
command: 61 00 00 00
# 
name: Movies
type: parsed
protocol: NEC
address: 04 00 00 00
command: 81 00 00 00
# 
name: Play
type: parsed
protocol: NEC
address: 04 00 00 00
command: B0 00 00 00
# 
name: Pause
type: parsed
protocol: NEC
address: 04 00 00 00
command: BA 00 00 00
