Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: BRIGHTNESS_+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: BRIGHTNESS_-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 13 00 00 00
#
name: COLOR_+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 14 00 00 00
#
name: COLOR_-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: BASS_+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 16 00 00 00
#
name: BASS_-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 17 00 00 00
#
name: TREBLE_+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 18 00 00 00
#
name: TREBLE_-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 19 00 00 00
#
name: BALANCE_+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1A 00 00 00
#
name: BALANCE_-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1B 00 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1B 00 00 00
#
name: CONTRAST_+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1C 00 00 00
#
name: CONTRAST_-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1D 00 00 00
#
name: TINT_-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1F 00 00 00
#
name: TINT_+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 27 00 00 00
#
name: ?
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2F 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 30 00 00 00
#
name: PHASE_+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 48 00 00 00
#
name: PHASE_-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 49 00 00 00
#
name: SHARPNESS_+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4D 00 00 00
#
name: SHARPNESS_-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4E 00 00 00
#
name: ^
type: parsed
protocol: NECext
address: 00 00 00 00
command: 50 00 00 00
#
name: V
type: parsed
protocol: NECext
address: 00 00 00 00
command: 51 00 00 00
#
name: ADJUST
type: parsed
protocol: NECext
address: 00 00 00 00
command: 52 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 53 00 00 00
#
name: <
type: parsed
protocol: NECext
address: 00 00 00 00
command: 55 00 00 00
#
name: >
type: parsed
protocol: NECext
address: 00 00 00 00
command: 56 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 57 00 00 00
#
name: *
type: parsed
protocol: NECext
address: 00 00 00 00
command: 77 00 00 00
