Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 04 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 04 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 04 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 04 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 04 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 04 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 04 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 04 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 04 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 04 00 00 00
command: 09 00 00 00
#
name: Off
type: parsed
protocol: NECext
address: 04 00 00 00
command: 0C 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 04 00 00 00
command: 0F 00 00 00
#
name: Shuffle
type: parsed
protocol: NECext
address: 04 00 00 00
command: 1C 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 04 00 00 00
command: 1D 00 00 00
#
name: LAST
type: parsed
protocol: NECext
address: 04 00 00 00
command: 20 00 00 00
#
name: First
type: parsed
protocol: NECext
address: 04 00 00 00
command: 21 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 04 00 00 00
command: 2C 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 04 00 00 00
command: 30 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 04 00 00 00
command: 31 00 00 00
#
name: RepeatA-B
type: parsed
protocol: NECext
address: 04 00 00 00
command: 3B 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 04 00 00 00
command: 4B 00 00 00
#
name: LANGUAGE
type: parsed
protocol: NECext
address: 04 00 00 00
command: 4E 00 00 00
#
name: DVD
type: parsed
protocol: NECext
address: 04 00 00 00
command: 54 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 04 00 00 00
command: 58 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 04 00 00 00
command: 59 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 5A 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 04 00 00 00
command: 5B 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 04 00 00 00
command: 5C 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 04 00 00 00
command: 83 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: 04 00 00 00
command: 85 00 00 00
#
name: T-C
type: parsed
protocol: NECext
address: 04 00 00 00
command: C8 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 04 00 00 00
command: F7 00 00 00
