Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 30 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 31 00 00 00
#
name: TR_PLAY
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 31 00 00 00
#
name: SCAN<<
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 32 00 00 00
#
name: SCAN_BACK
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 32 00 00 00
#
name: SCAN_-
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 32 00 00 00
#
name: TR_SCAN_<<
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 32 00 00 00
#
name: SCAN>>
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 33 00 00 00
#
name: SCAN_FORWARD
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 33 00 00 00
#
name: SCAN_+
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 33 00 00 00
#
name: TR_SCAN_>>
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 33 00 00 00
#
name: TRACK_>>
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 34 00 00 00
#
name: TRACK_FORWARD
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 34 00 00 00
#
name: TRACK_+
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 34 00 00 00
#
name: TR_SKIP_>>
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 34 00 00 00
#
name: TRACK_<<
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 35 00 00 00
#
name: TRACK_BACK
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 35 00 00 00
#
name: TRACK_-
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 35 00 00 00
#
name: TR_SKIP_<<
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 35 00 00 00
#
name: OPEN/CLOSE
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 36 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 38 00 00 00
#
name: TR_PAUSE
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 38 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 39 00 00 00
#
name: TR_STOP
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 39 00 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 39 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 3A 00 00 00
#
name: INFO/DISPLAY
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 3A 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 3B 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 3C 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 3D 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 3E 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 3F 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 40 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 41 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 42 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 43 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 44 00 00 00
#
name: RETURN
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 45 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 46 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 47 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 48 00 00 00
#
name: TITLE
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 4A 00 00 00
#
name: TITLE/POPUP
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 4A 00 00 00
#
name: TITLE/POP_UP
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 4A 00 00 00
#
name: TITLE/PUPUP
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 4A 00 00 00
#
name: DISC_MENU
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 4B 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 4C 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 4F 00 00 00
#
name: AUDIO_MODE
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 4F 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 50 00 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 53 00 00 00
#
name: A-B
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 55 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 56 00 00 00
#
name: CURSOR_ENTER
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 58 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 59 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 5A 00 00 00
#
name: VIDEO_PIP
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 5F 00 00 00
#
name: MARKER
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 61 00 00 00
#
name: SEARCH
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 62 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 64 00 00 00
#
name: HOME
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 67 00 00 00
#
name: POWER_ON
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 75 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 76 00 00 00
#
name: LOCK
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 79 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7C 00 00 00
#
name: A_(RED)
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7C 00 00 00
#
name: RED_-_A
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7C 00 00 00
#
name: COLOR_1_RED
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7C 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7D 00 00 00
#
name: B_(GREEN)
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7D 00 00 00
#
name: GREEN_-_B
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7D 00 00 00
#
name: COLOR_2_GREEN
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7D 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7E 00 00 00
#
name: C_(YELLOW)
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7E 00 00 00
#
name: YELLOW_-_C
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7E 00 00 00
#
name: COLOR_3_YELLOW
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7E 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7F 00 00 00
#
name: D_(BLUE)
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7F 00 00 00
#
name: BLUE_-_D
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7F 00 00 00
#
name: COLOR_4_BLUE
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: 7F 00 00 00
#
name: CURSOR
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: C0 00 00 00
#
name: CURSOR_LEFT_UP
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: C1 00 00 00
#
name: CURSOR_RIGHT_UP
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: C2 00 00 00
#
name: CURSOR_LEFT_DOWN
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: C3 00 00 00
#
name: CURSOR_RIGHT_DOWN
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: C4 00 00 00
#
name: RESOLUTION
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: F5 00 00 00
#
name: POP_UP
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: F6 00 00 00
#
name: SUBTITLE_ON/OFF
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: F7 00 00 00
#
name: RESUME_PLAY
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: F8 00 00 00
#
name: MUSIC_ID
type: parsed
protocol: NECext
address: 2D 2D 00 00
command: FA 00 00 00
