Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 09 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 0C 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 13 00 00 00
#
name: LAST
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 14 00 00 00
#
name: MYSHOWS
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 15 00 00 00
#
name: THUMBSDOWN
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 16 00 00 00
#
name: THUMBSUP
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 17 00 00 00
#
name: SLOW
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 18 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 19 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 1A 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 20 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 21 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 22 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 2A 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 2B 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 2F 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 30 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 32 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 34 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 36 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 37 00 00 00
#
name: HOME
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 4F 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 50 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 51 00 00 00
#
name: EPG
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 52 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 53 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 55 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 56 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 57 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6A 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6B 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6C 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6D 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 0A 00 00 00
command: 6E 00 00 00
