Filetype: IR signals file
Version: 1
#
name: LEFTARROW
type: parsed
protocol: NECext
address: 40 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 40 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 40 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 40 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 40 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 40 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 40 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 40 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 40 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 40 00 00 00
command: 09 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 40 00 00 00
command: 0A 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 40 00 00 00
command: 0C 00 00 00
#
name: COLOR
type: parsed
protocol: NECext
address: 40 00 00 00
command: 0D 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 40 00 00 00
command: 0E 00 00 00
#
name: F11
type: parsed
protocol: NECext
address: 40 00 00 00
command: 0F 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 40 00 00 00
command: 10 00 00 00
#
name: CAPTURE
type: parsed
protocol: NECext
address: 40 00 00 00
command: 11 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 40 00 00 00
command: 12 00 00 00
#
name: LOOP
type: parsed
protocol: NECext
address: 40 00 00 00
command: 13 00 00 00
#
name: FREEZE
type: parsed
protocol: NECext
address: 40 00 00 00
command: 14 00 00 00
#
name: RADIO
type: parsed
protocol: NECext
address: 40 00 00 00
command: 15 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 40 00 00 00
command: 16 00 00 00
#
name: RIGHTARROW
type: parsed
protocol: NECext
address: 40 00 00 00
command: 17 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 40 00 00 00
command: 18 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 40 00 00 00
command: 19 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1A 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1B 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1C 00 00 00
#
name: AUTOSCAN
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1D 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1E 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 40 00 00 00
command: 1F 00 00 00
