Filetype: IR signals file
Version: 1
# 
# Hisense EN3Y39H TV
# 
name: POWER
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 0D F2 00 00
# 
name: Input
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 12 ED 00 00
# 
name: VOL+
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 44 BB 00 00
# 
name: VOL-
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 43 BC 00 00
# 
name: CH+
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 4A B5 00 00
# 
name: CH-
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 4B B4 00 00
# 
name: Nav_up
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 16 E9 00 00
# 
name: Nav_dn
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 17 E8 00 00
# 
name: Nav_lft
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 19 E6 00 00
# 
name: Nav_rgt
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 18 E7 00 00
# 
name: Nav_ok
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 15 EA 00 00
# 
name: Nav_setting
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 0F F0 00 00
# 
name: Nav_menu
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 14 EB 00 00
# 
name: Nav_back
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 48 B7 00 00
# 
name: Nav_exit
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 5C A3 00 00
# 
name: Num_1
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 01 FE 00 00
# 
name: Num_2
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 02 FD 00 00
# 
name: Num_3
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 03 FC 00 00
# 
name: Num_4
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 04 FB 00 00
# 
name: Num_5
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 05 FA 00 00
# 
name: Num_6
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 06 F9 00 00
# 
name: Num_7
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 07 F8 00 00
# 
name: Num_8
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 08 F7 00 00
# 
name: Num_9
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 09 F6 00 00
# 
name: Num_0
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 00 FF 00 00
# 
name: MUTE
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 0E F1 00 00
# 
name: Home
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 20 DF 00 00
# 
name: Red_A
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 52 AD 00 00
# 
name: Green_B
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 53 AC 00 00
# 
name: Yellow_C
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 54 AB 00 00
# 
name: Blue_D
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 55 AA 00 00
# 
name: Guide
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 3A C5 00 00
# 
name: Info
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 0C F3 00 00
# 
name: Sport
type: parsed
protocol: NECext
address: 00 BF 00 00
command: CF 30 00 00
# 
name: PMode
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 10 EF 00 00
# 
name: SMode
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 11 EE 00 00
# 
name: Sleep
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 1A E5 00 00
# 
name: ChList
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 21 DE 00 00
# 
name: Add_Rew
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 58 A7 00 00
# 
name: Add_Play
type: parsed
protocol: NECext
address: 00 BF 00 00
command: A8 57 00 00
# 
name: Add_Ffd
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 59 A6 00 00
# 
name: Add_Stop
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 5A A5 00 00
# 
name: Add_Pause
type: parsed
protocol: NECext
address: 00 BF 00 00
command: A9 56 00 00
# 
name: Add_Rec
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 5E A1 00 00
# 
name: Subtitle
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 1F E0 00 00
# 
name: Language
type: parsed
protocol: NECext
address: 00 BF 00 00
command: BC 43 00 00
# 
name: Txt
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 45 BA 00 00
# 
name: Fn_Menu
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 5F A0 00 00
# 
name: Fn_Youtube
type: parsed
protocol: NECext
address: 00 BF 00 00
command: AA 55 00 00
# 
name: Fn_Netflix
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 47 B8 00 00
# 
name: Fn_Media
type: parsed
protocol: NECext
address: 00 BF 00 00
command: 33 CC 00 00
