Filetype: IR signals file
Version: 1
# 
name: POWER
type: parsed
protocol: NECext
address: 86 05 00 00
command: 0F F0 00 00
# 
name: Ok
type: parsed
protocol: NECext
address: 86 05 00 00
command: 18 E7 00 00
# 
name: Up
type: parsed
protocol: NECext
address: 86 05 00 00
command: 42 BD 00 00
# 
name: Down
type: parsed
protocol: NECext
address: 86 05 00 00
command: 43 BC 00 00
# 
name: Left
type: parsed
protocol: NECext
address: 86 05 00 00
command: 16 E9 00 00
# 
name: Right
type: parsed
protocol: NECext
address: 86 05 00 00
command: 15 EA 00 00
# 
name: VOL+
type: parsed
protocol: NECext
address: 86 05 00 00
command: 0C F3 00 00
# 
name: V_down
type: parsed
protocol: NECext
address: 86 05 00 00
command: 0D F2 00 00
# 
name: Back
type: parsed
protocol: NECext
address: 86 05 00 00
command: 1B E4 00 00
# 
name: Home
type: parsed
protocol: NECext
address: 86 05 00 00
command: 14 EB 00 00
# 
name: MUTE
type: parsed
protocol: NEC
address: 04 00 00 00
command: 09 00 00 00
# 
name: Netflix
type: parsed
protocol: NEC
address: 04 00 00 00
command: 4C 00 00 00
# 
name: Hulu
type: parsed
protocol: NEC
address: 04 00 00 00
command: 5C 00 00 00
# 
name: Sleep
type: parsed
protocol: NEC
address: 04 00 00 00
command: 1A 00 00 00
# 
name: Opt
type: parsed
protocol: NEC
address: 04 00 00 00
command: 0C 00 00 00
# 
name: Return
type: parsed
protocol: NEC
address: 04 00 00 00
command: 41 00 00 00
# 
name: Seek_fwd
type: parsed
protocol: NEC
address: 04 00 00 00
command: 5B 00 00 00
# 
name: Rewind
type: parsed
protocol: NEC
address: 04 00 00 00
command: 4F 00 00 00
# 
name: Play
type: parsed
protocol: NEC
address: 04 00 00 00
command: 42 00 00 00
