Filetype: IR signals file
Version: 1
#
name: PLAYPAUSE
type: parsed
protocol: NECext
address: 81 81 00 00
command: 01 00 00 00
#
name: Preset_Repeat
type: parsed
protocol: NECext
address: 81 81 00 00
command: 02 00 00 00
#
name: Snooze
type: parsed
protocol: NECext
address: 81 81 00 00
command: 03 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 81 81 00 00
command: 04 00 00 00
#
name: Stop_Band
type: parsed
protocol: NECext
address: 81 81 00 00
command: 09 00 00 00
#
name: Intro
type: parsed
protocol: NECext
address: 81 81 00 00
command: 0A 00 00 00
#
name: Timer
type: parsed
protocol: NECext
address: 81 81 00 00
command: 0B 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 81 81 00 00
command: 11 00 00 00
#
name: Random
type: parsed
protocol: NECext
address: 81 81 00 00
command: 12 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 81 81 00 00
command: 13 00 00 00
#
name: X-Bass
type: parsed
protocol: NECext
address: 81 81 00 00
command: 14 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 81 81 00 00
command: 17 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 81 81 00 00
command: 19 00 00 00
#
name: Mem
type: parsed
protocol: NECext
address: 81 81 00 00
command: 1A 00 00 00
#
name: Display
type: parsed
protocol: NECext
address: 81 81 00 00
command: 1B 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 81 81 00 00
command: 1F 00 00 00
#
name: Function
type: parsed
protocol: NECext
address: 81 81 00 00
command: 20 00 00 00
