Filetype: IR signals file
Version: 1
#
name: DVD
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 03 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 04 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 05 00 00 00
#
name: skip_scan_down
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 06 00 00 00
#
name: skip_scan_up
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 07 00 00 00
#
name: pr_preset_down
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 12 00 00 00
#
name: pr_preset_up
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 13 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 16 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 17 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 1E 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 1F 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 41 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 42 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 43 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 44 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 45 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 46 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 47 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 48 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 49 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 4B 00 00 00
#
name: program
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 4D 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 4E 00 00 00
#
name: pause_step
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 4F 00 00 00
#
name: band
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 59 00 00 00
#
name: dimmer
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 5E 00 00 00
#
name: exit_cancel
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 69 00 00 00
#
name: caption
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 6A 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 6B 00 00 00
#
name: i_ii
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 7A 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 7B 00 00 00
#
name: tv_radio
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 82 00 00 00
#
name: AUX
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 8A 00 00 00
#
name: OPEN
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: 9A 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: A0 00 00 00
#
name: sound
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: A1 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: A2 00 00 00
#
name: display
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: A3 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: A4 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: A5 00 00 00
#
name: s_title
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: AB 00 00 00
#
name: repeat_a-b
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: AD 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: AE 00 00 00
#
name: DVD
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: AF 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: B0 00 00 00
#
name: slow_scan_down
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: B1 00 00 00
#
name: slow_scan_up
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: B2 00 00 00
#
name: SEARCH
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: B3 00 00 00
#
name: marker
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: B4 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 2C 2C 00 00
command: C2 00 00 00
