Filetype: IR signals file
Version: 1
#
name: OFF
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 01 00 00 00
#
name: POWER_OFF
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 01 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 02 00 00 00
#
name: POWER_ON
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 02 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 03 00 00 00
#
name: V1
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 05 00 00 00
#
name: IN_1_VCR
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 05 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 06 00 00 00
#
name: IN_3_TV
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 06 00 00 00
#
name: IN_8
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 07 00 00 00
#
name: V2
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 09 00 00 00
#
name: IN_2_TIVO
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 09 00 00 00
#
name: TAPE
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 0B 00 00 00
#
name: IN_7_TAPE
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 0B 00 00 00
#
name: DVD
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 0D 00 00 00
#
name: IN_4_DVD
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 0D 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 0E 00 00 00
#
name: CD
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 0F 00 00 00
#
name: IN_5_CD
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 0F 00 00 00
#
name: BAND
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 13 00 00 00
#
name: CENTER_-
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 15 00 00 00
#
name: CENTER_+
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 16 00 00 00
#
name: STA_DN
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 17 00 00 00
#
name: STA_UP
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 18 00 00 00
#
name: REAR_-
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 19 00 00 00
#
name: REAR_+
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 1A 00 00 00
#
name: TUNE-
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 1B 00 00 00
#
name: TUNE_DN
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 1B 00 00 00
#
name: TUNE+
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 1C 00 00 00
#
name: TUNE_UP
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 1C 00 00 00
#
name: SUB_-
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 1D 00 00 00
#
name: SUB_+
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 1E 00 00 00
#
name: CR_LEFT
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 1F 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 1F 00 00 00
#
name: CR_RIGHT
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 20 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 20 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 23 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 24 00 00 00
#
name: MODE
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 26 00 00 00
#
name: 10+
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 29 00 00 00
#
name: EQ
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 2A 00 00 00
#
name: DVD-A
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 2B 00 00 00
#
name: CR_DOWN
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 2D 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 2D 00 00 00
#
name: CR_UP
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 2E 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 2E 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 2F 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 30 00 00 00
#
name: SELECT
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 30 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 31 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 32 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 33 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 33 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 35 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 36 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 37 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 37 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 39 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 3A 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 3B 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 3E 00 00 00
#
name: Z
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 3F 00 00 00
#
name: SAVE
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 40 00 00 00
#
name: SAT
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 4A 00 00 00
#
name: IN_6_SAT
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 4A 00 00 00
#
name: PRESET_+
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 4B 00 00 00
#
name: CHANNEL_+
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 4B 00 00 00
#
name: D_IN
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 5A 00 00 00
#
name: BASS-
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 65 00 00 00
#
name: BASS_DN
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 65 00 00 00
#
name: IN_9
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 6E 00 00 00
#
name: AM
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 76 00 00 00
#
name: AM_TUNER
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 76 00 00 00
#
name: TREBLE-
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 79 00 00 00
#
name: TREB_DN
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 79 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 7D 00 00 00
#
name: THX
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 8A 00 00 00
#
name: FM
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 8E 00 00 00
#
name: FM_MODE
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 8E 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 8E 00 00 00
#
name: MONO
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: 9A 00 00 00
#
name: POWER_TOGGLE
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: A2 00 00 00
#
name: PRESET_-
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: C6 00 00 00
#
name: CHANNEL_-
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: C6 00 00 00
#
name: SURR
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: CA 00 00 00
#
name: A_KEY
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: CF 00 00 00
#
name: LOUDNESS
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: CF 00 00 00
#
name: LOUD
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: CF 00 00 00
#
name: STEREO
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: E2 00 00 00
#
name: BASS+
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: E5 00 00 00
#
name: BASS_UP
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: E5 00 00 00
#
name: ST/MONO
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: EB 00 00 00
#
name: TREBLE+
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: F9 00 00 00
#
name: TREB_UP
type: parsed
protocol: NECext
address: 0B 4F 00 00
command: F9 00 00 00
