Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 08 00 00 00
command: 00 00 00 00
#
name: P/L
type: parsed
protocol: NECext
address: 08 00 00 00
command: 02 00 00 00
#
name: STORE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 03 00 00 00
#
name: V/H
type: parsed
protocol: NECext
address: 08 00 00 00
command: 04 00 00 00
#
name: J17
type: parsed
protocol: NECext
address: 08 00 00 00
command: 06 00 00 00
#
name: W/N
type: parsed
protocol: NECext
address: 08 00 00 00
command: 07 00 00 00
#
name: MODE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 08 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 08 00 00 00
command: 09 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0A 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0B 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0C 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0D 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0E 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0F 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 08 00 00 00
command: 10 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 08 00 00 00
command: 11 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 08 00 00 00
command: 12 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 08 00 00 00
command: 13 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 08 00 00 00
command: 14 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 15 00 00 00
#
name: A/B
type: parsed
protocol: NECext
address: 08 00 00 00
command: 19 00 00 00
