Filetype: IR signals file
Version: 1
# 
name: On
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 03 FC 00 00
# 
name: Off
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 02 FD 00 00
# 
name: Brightness_Down
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 01 FE 00 00
# 
name: Brightness_Up
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 00 FF 00 00
# 
name: White
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 07 F8 00 00
# 
name: Blue
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 06 F9 00 00
# 
name: Green
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 05 FA 00 00
# 
name: Red
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 04 FB 00 00
# 
name: Flash
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0B F4 00 00
# 
name: Strobe
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0F F0 00 00
# 
name: Fade
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 13 EC 00 00
# 
name: Holiday
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 17 E8 00 00
# 
name: Lighter_blue
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0A F5 00 00
# 
name: Purple
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0E F1 00 00
# 
name: Violet
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 12 ED 00 00
# 
name: Pink
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 16 E9 00 00
# 
name: Lime_Green
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 09 F6 00 00
# 
name: Cyan
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0D F2 00 00
# 
name: Lighter_Cyan
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 11 EE 00 00
# 
name: Turquoise
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 15 EA 00 00
# 
name: Lighter_red
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 08 F7 00 00
# 
name: India_Red
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 0C F3 00 00
# 
name: Orange
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 10 EF 00 00
# 
name: Yellow
type: parsed
protocol: NECext
address: 00 EF 00 00
command: 14 EB 00 00
