Filetype: IR signals file
Version: 1
#
name: TUNER_PRESET_NEXT
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 00 00 00 00
#
name: TUNER_PRESET_PREVIOUS
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 01 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 02 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 03 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 04 00 00 00
#
name: MUTING
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 05 00 00 00
#
name: INPUT_SELECTOR_LINE
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 06 00 00 00
#
name: INPUT_SELECTOR_TAPE-2
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 07 00 00 00
#
name: INPUT_SELECTOR_TAPE-1
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 08 00 00 00
#
name: INPUT_SELECTOR_CD
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 09 00 00 00
#
name: INPUT_SELECTOR_FM
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 0B 00 00 00
#
name: DECK-B_STOP
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 13 00 00 00
#
name: DECK-B_FORWARD_PLAY
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 15 00 00 00
#
name: DECK-B_REVERSE_PLAY
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 16 00 00 00
#
name: DECK-B_RECORD_PAUSE
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 18 00 00 00
#
name: DECK-B_FAST_FORWARD
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 19 00 00 00
#
name: DECK-B_FAST_REWIND
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1A 00 00 00
#
name: CD_PLAY
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1B 00 00 00
#
name: CD_STOP
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1C 00 00 00
#
name: CD_NEXT_TRACK
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1D 00 00 00
#
name: CD_PREVIOUS_TRACK
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1E 00 00 00
#
name: CD_PAUSE
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 1F 00 00 00
#
name: TUNER_GROUP
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 4A 00 00 00
#
name: DECK-A_STOP
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 4D 00 00 00
#
name: DECK-A_FORWARD_PLAY
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 4E 00 00 00
#
name: DECK-A_REVERSE_PLAY
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 4F 00 00 00
#
name: DECK-A_FAST_FORWARD
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 51 00 00 00
#
name: DECK-A_FAST_REWIND
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 52 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: D2 6D 00 00
command: 5D 00 00 00
