Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0C 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0D 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0E 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 0F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 10 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 11 00 00 00
#
name: PAGEUP
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 12 00 00 00
#
name: PAGEDOWN
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 13 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 14 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 15 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 19 00 00 00
#
name: BTN_FORWARD
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1A 00 00 00
#
name: BTN_BACK
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1B 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1E 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 1F 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 20 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 21 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 22 00 00 00
#
name: FIRST
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 23 00 00 00
#
name: MEDIA
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 24 00 00 00
#
name: PLAYPAUSE
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 6E 00 00 00
#
name: FAVORITES
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 80 00 00 00
#
name: SCREEN
type: parsed
protocol: NECext
address: 04 0F 00 00
command: 81 00 00 00
