Filetype: IR signals file
Version: 1
# 
# Sony RM-SCU37 Stereo Receiver
#
# Compatible with: CMT-BX30R, CMT-BX5, CMT-BX5BT, CMT-EH25
#                  CMT-EH26, CMT-FX205, CMT-NEZ50, HCD-CBX5
#                  HCD-EX600, MHC-EX600, MHC-EX700, MHC-EX900
# 
name: POWER
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 15 00 00 00
# 
name: Sleep
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 60 00 00 00
# 
name: Play
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 32 00 00 00
# 
name: Pause
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 39 00 00 00
# 
name: Stop
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 38 00 00 00
# 
name: Enter
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 7C 00 00 00
# 
name: VOL+
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 12 00 00 00
# 
name: VOL-
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 13 00 00 00
# 
name: |<<
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 30 00 00 00
# 
name: >>|
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 31 00 00 00
# 
name: <<
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 33 00 00 00
# 
name: >>
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 34 00 00 00
# 
name: Clear
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 0F 00 00 00
# 
name: EQ
type: parsed
protocol: SIRC15
address: 90 00 00 00
command: 63 00 00 00
# 
name: Dir-
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 2E 00 00 00
# 
name: Dir+
type: parsed
protocol: SIRC20
address: 3A 07 00 00
command: 2F 00 00 00
# 
name: Display
type: parsed
protocol: SIRC
address: 10 00 00 00
command: 4B 00 00 00
