Filetype: IR signals file
Version: 1
#
# BENQ DV3080
# Autogenerated from ircodes/BENQ/DV3080.xml
#
name: Unknown
type: parsed
protocol: NECext
address: F9 06 00 00
command: FF 00 00 00
#
name: INPUT
type: parsed
protocol: NECext
address: F9 06 00 00
command: 5D A2 00 00
#
name: INFO
type: parsed
protocol: NECext
address: F9 06 00 00
command: B5 4A 00 00
#
name: SLEEPTIMER
type: parsed
protocol: NECext
address: F9 06 00 00
command: E5 1A 00 00
#
name: SOUND
type: parsed
protocol: NECext
address: F9 06 00 00
command: 95 6A 00 00
#
name: AUDIOMODE
type: parsed
protocol: NECext
address: F9 06 00 00
command: 35 CA 00 00
#
name: TTX DISPLAY
type: parsed
protocol: NECext
address: F9 06 00 00
command: 0D F2 00 00
#
name: TTX INDEX
type: parsed
protocol: NECext
address: F9 06 00 00
command: CD 32 00 00
#
name: TTX INFO
type: parsed
protocol: NECext
address: F9 06 00 00
command: 8D 72 00 00
#
name: TTX SUBP
type: parsed
protocol: NECext
address: F9 06 00 00
command: 4D B2 00 00
#
name: TTX
type: parsed
protocol: NECext
address: F9 06 00 00
command: B7 48 00 00
#
name: PIP
type: parsed
protocol: NECext
address: F9 06 00 00
command: F7 08 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: F9 06 00 00
command: 67 98 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: F9 06 00 00
command: DD 22 00 00
#
name: CH+
type: parsed
protocol: NECext
address: F9 06 00 00
command: C5 3A 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: F9 06 00 00
command: C7 38 00 00
#
name: OK
type: parsed
protocol: NECext
address: F9 06 00 00
command: 75 8A 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: F9 06 00 00
command: ED 12 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: F9 06 00 00
command: 57 A8 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: F9 06 00 00
command: 47 B8 00 00
#
name: CH-
type: parsed
protocol: NECext
address: F9 06 00 00
command: D7 28 00 00
#
name: FREEZE
type: parsed
protocol: NECext
address: F9 06 00 00
command: 77 88 00 00
#
name: ASPECT
type: parsed
protocol: NECext
address: F9 06 00 00
command: 37 C8 00 00
#
name: MENU
type: parsed
protocol: NECext
address: F9 06 00 00
command: 3D C2 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: F9 06 00 00
command: BD 42 00 00
#
name: ZAP
type: parsed
protocol: NECext
address: F9 06 00 00
command: 0F F0 00 00
#
name: DUAL DIGIT
type: parsed
protocol: NECext
address: F9 06 00 00
command: 4F B0 00 00
#
name: 1
type: parsed
protocol: NECext
address: F9 06 00 00
command: DF 20 00 00
#
name: 2
type: parsed
protocol: NECext
address: F9 06 00 00
command: 5F A0 00 00
#
name: 3
type: parsed
protocol: NECext
address: F9 06 00 00
command: 05 FA 00 00
#
name: 4
type: parsed
protocol: NECext
address: F9 06 00 00
command: 1F E0 00 00
#
name: 5
type: parsed
protocol: NECext
address: F9 06 00 00
command: EF 10 00 00
#
name: 6
type: parsed
protocol: NECext
address: F9 06 00 00
command: 6F 90 00 00
#
name: 7
type: parsed
protocol: NECext
address: F9 06 00 00
command: AF 50 00 00
#
name: 8
type: parsed
protocol: NECext
address: F9 06 00 00
command: 2F D0 00 00
#
name: 9
type: parsed
protocol: NECext
address: F9 06 00 00
command: CF 30 00 00
#
name: BACKLIGHT
type: parsed
protocol: NECext
address: F9 06 00 00
command: D5 2A 00 00
#
name: 0
type: parsed
protocol: NECext
address: F9 06 00 00
command: 3F C0 00 00
#
name: USERSITUATION
type: parsed
protocol: NECext
address: F9 06 00 00
command: 55 AA 00 00
