Filetype: IR signals file
Version: 1
# 
name: POWER
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0C 00 00 00
# 
name: IpadPwr
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0D 00 00 00
# 
name: MUTE
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1E 00 00 00
# 
name: Alarm
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1F 00 00 00
# 
name: Clock
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1C 00 00 00
# 
name: Sleep
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1D 00 00 00
# 
name: Repeat
type: parsed
protocol: NEC
address: 00 00 00 00
command: 09 00 00 00
# 
name: Bass_dwn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 14 00 00 00
# 
name: Bass_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 15 00 00 00
# 
name: Video
type: parsed
protocol: NEC
address: 00 00 00 00
command: 16 00 00 00
# 
name: Trebble_dwn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 17 00 00 00
# 
name: Trebble_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 18 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: 00 00 00 00
command: 00 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: 00 00 00 00
command: 01 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: 00 00 00 00
command: 02 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: 00 00 00 00
command: 03 00 00 00
# 
name: 5
type: parsed
protocol: NEC
address: 00 00 00 00
command: 04 00 00 00
# 
name: 6
type: parsed
protocol: NEC
address: 00 00 00 00
command: 05 00 00 00
# 
name: 7
type: parsed
protocol: NEC
address: 00 00 00 00
command: 06 00 00 00
# 
name: 8
type: parsed
protocol: NEC
address: 00 00 00 00
command: 07 00 00 00
# 
name: 9
type: parsed
protocol: NEC
address: 00 00 00 00
command: 08 00 00 00
# 
name: 0
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0A 00 00 00
# 
name: .
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0B 00 00 00
# 
name: Menu
type: parsed
protocol: NEC
address: 00 00 00 00
command: 19 00 00 00
# 
name: Shuffle
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1A 00 00 00
# 
name: EQ
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1B 00 00 00
# 
name: VOL+
type: parsed
protocol: NEC
address: 00 00 00 00
command: 42 00 00 00
# 
name: VOL-
type: parsed
protocol: NEC
address: 00 00 00 00
command: 43 00 00 00
# 
name: Skip_forward
type: parsed
protocol: NEC
address: 00 00 00 00
command: 40 00 00 00
# 
name: Rewind
type: parsed
protocol: NEC
address: 00 00 00 00
command: 41 00 00 00
# 
name: Stop
type: parsed
protocol: NEC
address: 00 00 00 00
command: 45 00 00 00
# 
name: Play/Pause
type: parsed
protocol: NEC
address: 00 00 00 00
command: 44 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 10 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: 00 00 00 00
command: 11 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: 00 00 00 00
command: 13 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: 00 00 00 00
command: 12 00 00 00
# 
name: Select
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0E 00 00 00
# 
name: Album_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 48 00 00 00
# 
name: Album_dwn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 4C 00 00 00
# 
name: Chapter_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 49 00 00 00
# 
name: Chapter_dwn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 4D 00 00 00
# 
name: Memory_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 4A 00 00 00
# 
name: Memory_dwn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 4E 00 00 00
# 
name: Playlist_up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 4B 00 00 00
# 
name: Playlist_dwn
type: parsed
protocol: NEC
address: 00 00 00 00
command: 4F 00 00 00
# 
name: Source
type: parsed
protocol: NEC
address: 00 00 00 00
command: 50 00 00 00
# 
name: Display
type: parsed
protocol: NEC
address: 00 00 00 00
command: 51 00 00 00
# 
name: Mem
type: parsed
protocol: NEC
address: 00 00 00 00
command: 52 00 00 00
# 
name: Ipod
type: parsed
protocol: NEC
address: 00 00 00 00
command: 53 00 00 00
