Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 09 00 00 00
#
name: STANDBYON
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 20 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 22 00 00 00
#
name: COLORSYSTEM
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 2E 00 00 00
#
name: INPUTSELECT
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 40 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 50 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 51 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 60 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 61 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 64 00 00 00
#
name: SOUNDSELECT
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 65 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 70 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 73 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 74 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 75 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 76 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 77 00 00 00
#
name: PROGRETURN
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 78 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 79 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 7A 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 7B 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 7C 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 7D 00 00 00
#
name: SCREENMODE
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 90 00 00 00
#
name: PIP
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 91 00 00 00
#
name: DISP
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 9B 00 00 00
#
name: EXPAND
type: parsed
protocol: NECext
address: 84 E0 00 00
command: 9D 00 00 00
#
name: TXT
type: parsed
protocol: NECext
address: 84 E0 00 00
command: A8 00 00 00
#
name: REVEAL
type: parsed
protocol: NECext
address: 84 E0 00 00
command: A9 00 00 00
#
name: TXTSTOPSEQUENCE
type: parsed
protocol: NECext
address: 84 E0 00 00
command: AA 00 00 00
#
name: SUBCODE
type: parsed
protocol: NECext
address: 84 E0 00 00
command: AD 00 00 00
#
name: TXTCONTENTSPAGE
type: parsed
protocol: NECext
address: 84 E0 00 00
command: AE 00 00 00
#
name: SERVICE
type: parsed
protocol: NECext
address: 84 E0 00 00
command: FF 00 00 00
