Filetype: IR signals file
Version: 1
#
name: TV_POWER
type: parsed
protocol: NECext
address: 47 00 00 00
command: 02 00 00 00
#
name: TV_VOL_+
type: parsed
protocol: NECext
address: 47 00 00 00
command: 22 00 00 00
#
name: TV_VOL_-
type: parsed
protocol: NECext
address: 47 00 00 00
command: 2A 00 00 00
#
name: TV_INPUT
type: parsed
protocol: NECext
address: 47 00 00 00
command: 3A 00 00 00
