Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 67 00 00 00
command: 00 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 67 00 00 00
command: 01 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 67 00 00 00
command: 02 00 00 00
#
name: PLAY_>
type: parsed
protocol: NECext
address: 67 00 00 00
command: 04 00 00 00
#
name: LAST_PLAY
type: parsed
protocol: NECext
address: 67 00 00 00
command: 05 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 67 00 00 00
command: 08 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 67 00 00 00
command: 09 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 67 00 00 00
command: 0B 00 00 00
#
name: MEMORY
type: parsed
protocol: NECext
address: 67 00 00 00
command: 0C 00 00 00
#
name: T/C
type: parsed
protocol: NECext
address: 67 00 00 00
command: 0F 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 67 00 00 00
command: 10 00 00 00
#
name: STOP_[]
type: parsed
protocol: NECext
address: 67 00 00 00
command: 14 00 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: 67 00 00 00
command: 17 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 67 00 00 00
command: 18 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 67 00 00 00
command: 1B 00 00 00
#
name: PAUSE_
type: parsed
protocol: NECext
address: 67 00 00 00
command: 1C 00 00 00
#
name: +10
type: parsed
protocol: NECext
address: 67 00 00 00
command: 1E 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 67 00 00 00
command: 20 00 00 00
#
name: SKIP_>>
type: parsed
protocol: NECext
address: 67 00 00 00
command: 24 00 00 00
#
name: FWD_>>
type: parsed
protocol: NECext
address: 67 00 00 00
command: 25 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 67 00 00 00
command: 28 00 00 00
#
name: SKIP_<<
type: parsed
protocol: NECext
address: 67 00 00 00
command: 2C 00 00 00
#
name: REV_<<
type: parsed
protocol: NECext
address: 67 00 00 00
command: 2D 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 67 00 00 00
command: 30 00 00 00
#
name: SLOW_>
type: parsed
protocol: NECext
address: 67 00 00 00
command: 34 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 67 00 00 00
command: 35 00 00 00
#
name: OPEN/CLOSE
type: parsed
protocol: NECext
address: 67 00 00 00
command: 36 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 67 00 00 00
command: 38 00 00 00
#
name: A-B_REPEAT
type: parsed
protocol: NECext
address: 67 00 00 00
command: 3D 00 00 00
#
name: RANDOM
type: parsed
protocol: NECext
address: 67 00 00 00
command: 3E 00 00 00
#
name: TITLE
type: parsed
protocol: NECext
address: 67 00 00 00
command: 40 00 00 00
#
name: CURSOR_^
type: parsed
protocol: NECext
address: 67 00 00 00
command: 41 00 00 00
#
name: CURSOR_V
type: parsed
protocol: NECext
address: 67 00 00 00
command: 49 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 67 00 00 00
command: 50 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 67 00 00 00
command: 52 00 00 00
#
name: SET_UP
type: parsed
protocol: NECext
address: 67 00 00 00
command: 60 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 67 00 00 00
command: 63 00 00 00
#
name: ANGLE
type: parsed
protocol: NECext
address: 67 00 00 00
command: 64 00 00 00
#
name: CURSOR_<
type: parsed
protocol: NECext
address: 67 00 00 00
command: 65 00 00 00
#
name: SUBTITLE_ON_OFF
type: parsed
protocol: NECext
address: 67 00 00 00
command: 67 00 00 00
#
name: CURSOR_>
type: parsed
protocol: NECext
address: 67 00 00 00
command: 6D 00 00 00
#
name: RETURN
type: parsed
protocol: NECext
address: 67 00 00 00
command: 6F 00 00 00
