Filetype: IR signals file
Version: 1
#
# TOPFIELD TF7700HSCI
# Autogenerated from ircodes/TOPFIELD/TF7700HSCI.xml
#
name: POWER
type: parsed
protocol: NECext
address: F3 0C 00 00
command: AF 50 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: F3 0C 00 00
command: CF 30 00 00
#
name: TV/SAT
type: parsed
protocol: NECext
address: F3 0C 00 00
command: DF 20 00 00
#
name: 1
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 77 88 00 00
#
name: 2
type: parsed
protocol: NECext
address: F3 0C 00 00
command: B7 48 00 00
#
name: 3
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 37 C8 00 00
#
name: 4
type: parsed
protocol: NECext
address: F3 0C 00 00
command: D7 28 00 00
#
name: 5
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 57 A8 00 00
#
name: 6
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 97 68 00 00
#
name: 7
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 17 E8 00 00
#
name: 8
type: parsed
protocol: NECext
address: F3 0C 00 00
command: E7 18 00 00
#
name: 9
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 67 98 00 00
#
name: EPG
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 27 D8 00 00
#
name: 0
type: parsed
protocol: NECext
address: F3 0C 00 00
command: F7 08 00 00
#
name: FAV
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 6F 90 00 00
#
name: Audio
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 5D A2 00 00
#
name: CH
type: parsed
protocol: NECext
address: F3 0C 00 00
command: FF 00 00 00
#
name: Video
type: parsed
protocol: NECext
address: F3 0C 00 00
command: EF 10 00 00
#
name: VOL
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 3F C0 00 00
#
name: OK
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 07 F8 00 00
#
name: VOL
type: parsed
protocol: NECext
address: F3 0C 00 00
command: BF 40 00 00
#
name: Menu
type: parsed
protocol: NECext
address: F3 0C 00 00
command: A7 58 00 00
#
name: CH
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 7F 80 00 00
#
name: Text
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 1D E2 00 00
#
name: Exit
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 05 FA 00 00
#
name: Display
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 47 B8 00 00
#
name: TV
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 3D C2 00 00
#
name: Sleep Timer
type: parsed
protocol: NECext
address: F3 0C 00 00
command: DD 22 00 00
#
name: Subt List
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 1F E0 00 00
#
name: Zoom
type: parsed
protocol: NECext
address: F3 0C 00 00
command: C9 36 00 00
#
name: Back
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 87 78 00 00
#
name: Epg
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 49 B6 00 00
#
name: Opt?
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 89 76 00 00
#
name: App
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 69 96 00 00
#
name: Info
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 59 A6 00 00
#
name: R
type: parsed
protocol: NECext
address: F3 0C 00 00
command: E9 16 00 00
#
name: G
type: parsed
protocol: NECext
address: F3 0C 00 00
command: D9 26 00 00
#
name: Y
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 99 66 00 00
#
name: B
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 19 E6 00 00
#
name: F1
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 5F A0 00 00
#
name: F2
type: parsed
protocol: NECext
address: F3 0C 00 00
command: A9 56 00 00
#
name: F3
type: parsed
protocol: NECext
address: F3 0C 00 00
command: F9 06 00 00
#
name: F4
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 79 86 00 00
#
name: F5
type: parsed
protocol: NECext
address: F3 0C 00 00
command: B9 46 00 00
#
name: F6
type: parsed
protocol: NECext
address: F3 0C 00 00
command: 39 C6 00 00
