Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: 1-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: Brightness_up
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: Brightness_down
type: parsed
protocol: NECext
address: 00 00 00 00
command: 13 00 00 00
#
name: Contrast_up
type: parsed
protocol: NECext
address: 00 00 00 00
command: 14 00 00 00
#
name: Contrast_down
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: Search_programm
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1E 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 00 00 00 00
command: 28 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 29 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2A 00 00 00
#
name: Skip_back
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2C 00 00 00
#
name: Skip_forw
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2E 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2F 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 00 00 00 00
command: 33 00 00 00
#
name: Forw
type: parsed
protocol: NECext
address: 00 00 00 00
command: 35 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 36 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 37 00 00 00
