Filetype: IR signals file
Version: 1
#
name: but_8
type: parsed
protocol: NECext
address: 50 00 00 00
command: 04 00 00 00
#
name: but_9
type: parsed
protocol: NECext
address: 50 00 00 00
command: 05 00 00 00
#
name: tv/video
type: parsed
protocol: NECext
address: 50 00 00 00
command: 09 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 50 00 00 00
command: 0B 00 00 00
#
name: but_10
type: parsed
protocol: NECext
address: 50 00 00 00
command: 0C 00 00 00
#
name: but_1
type: parsed
protocol: NECext
address: 50 00 00 00
command: 0D 00 00 00
#
name: but_2
type: parsed
protocol: NECext
address: 50 00 00 00
command: 0E 00 00 00
#
name: but_3
type: parsed
protocol: NECext
address: 50 00 00 00
command: 0F 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 50 00 00 00
command: 10 00 00 00
#
name: timer
type: parsed
protocol: NECext
address: 50 00 00 00
command: 11 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 50 00 00 00
command: 12 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 50 00 00 00
command: 15 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 50 00 00 00
command: 17 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 50 00 00 00
command: 18 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 50 00 00 00
command: 19 00 00 00
#
name: but_4
type: parsed
protocol: NECext
address: 50 00 00 00
command: 1C 00 00 00
#
name: but_5
type: parsed
protocol: NECext
address: 50 00 00 00
command: 1D 00 00 00
#
name: but_6
type: parsed
protocol: NECext
address: 50 00 00 00
command: 1E 00 00 00
#
name: but_7
type: parsed
protocol: NECext
address: 50 00 00 00
command: 1F 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 50 00 00 00
command: 44 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 50 00 00 00
command: 53 00 00 00
#
name: krasn
type: parsed
protocol: NECext
address: 50 00 00 00
command: 5B 00 00 00
#
name: zelen
type: parsed
protocol: NECext
address: 50 00 00 00
command: 5C 00 00 00
#
name: jolt
type: parsed
protocol: NECext
address: 50 00 00 00
command: 5D 00 00 00
#
name: zelen
type: parsed
protocol: NECext
address: 50 00 00 00
command: 5E 00 00 00
