Filetype: IR signals file
Version: 1
#
name: SPK+
type: parsed
protocol: NECext
address: 18 00 00 00
command: 00 00 00 00
#
name: SPK-
type: parsed
protocol: NECext
address: 18 00 00 00
command: 04 00 00 00
#
name: INPUT
type: parsed
protocol: NECext
address: 18 00 00 00
command: 08 00 00 00
#
name: SPK
type: parsed
protocol: NECext
address: 18 00 00 00
command: 0C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 18 00 00 00
command: 0D 00 00 00
#
name: S.BASS
type: parsed
protocol: NECext
address: 18 00 00 00
command: 10 00 00 00
#
name: EQ+
type: parsed
protocol: NECext
address: 18 00 00 00
command: 11 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 18 00 00 00
command: 14 00 00 00
#
name: EQ-
type: parsed
protocol: NECext
address: 18 00 00 00
command: 15 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 18 00 00 00
command: 18 00 00 00
#
name: EQ
type: parsed
protocol: NECext
address: 18 00 00 00
command: 19 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 18 00 00 00
command: 1C 00 00 00
#
name: MODE
type: parsed
protocol: NECext
address: 18 00 00 00
command: 1D 00 00 00
