Filetype: IR signals file
Version: 1
#
name: Unknown
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 00 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 00 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 01 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 02 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 03 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 05 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 06 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 07 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 09 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 0A 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 0B 00 00 00
#
name: CHANNEL_+
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 0D 00 00 00
#
name: CHANNEL_-
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 0E 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 0F 00 00 00
#
name: EDIT
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 10 00 00 00
#
name: SKIP_>>
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 13 00 00 00
#
name: TIMER
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 14 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 17 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 18 00 00 00
#
name: INPUT
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 1C 00 00 00
#
name: SCAN_>>
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 1F 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 40 00 00 00
#
name: DISC_MENU
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 41 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 42 00 00 00
#
name: PLAY_OPTIONS
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 43 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 47 00 00 00
#
name: CURSOR_ENTER
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 4A 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 4B 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 4C 00 00 00
#
name: TITLE
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 4D 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 4E 00 00 00
#
name: GUIDER
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 4F 00 00 00
#
name: SKIP_<<
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 50 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 54 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 55 00 00 00
#
name: SCAN_<<
type: parsed
protocol: NECext
address: 0A F7 00 00
command: 5C 00 00 00
