Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: 102ND
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: P
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: C
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 14 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: PIP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1B 00 00 00
#
name: N
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1C 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 00 00 00 00
command: 20 00 00 00
#
name: TXT_LANG
type: parsed
protocol: NECext
address: 00 00 00 00
command: 21 00 00 00
#
name: S
type: parsed
protocol: NECext
address: 00 00 00 00
command: 26 00 00 00
#
name: TXT_STOP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 29 00 00 00
#
name: TXT_TIME
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2A 00 00 00
#
name: TXT_MAGN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2B 00 00 00
#
name: TXT_REV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2C 00 00 00
#
name: TXT_X
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2D 00 00 00
#
name: TXT_MIX
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2E 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 00 00 00 00
command: 32 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 34 00 00 00
#
name: TXT_INFO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 35 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 36 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 00 00 00 00
command: 37 00 00 00
#
name: AV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 38 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3C 00 00 00
#
name: A
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3F 00 00 00
