Filetype: IR signals file
Version: 1
#
name: PLAY/PAUSE
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 00 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 01 00 00 00
#
name: PREVIOUS_TRACK
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 02 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 03 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 05 00 00 00
#
name: PAGE_-
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 06 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 07 00 00 00
#
name: NEXT_TRACK
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 08 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 09 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 0A 00 00 00
#
name: CURSOR_SELECT
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 0B 00 00 00
#
name: PAGE_+
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 0C 00 00 00
#
name: SETTINGS
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 0F 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 10 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 18 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: D4 BE 00 00
command: 1F 00 00 00
