Filetype: IR signals file
Version: 1
# 
# Yamaha Amplifier AX-396
#
name: POWER
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 1F 00 00 00
# 
name: VOL+
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 1A 00 00 00
# 
name: VOL-
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 1B 00 00 00
#
name: MD
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 19 00 00 00
# 
name: TAPE
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 18 00 00 00
# 
name: CD_DVD
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 15 00 00 00
# 
name: AUX
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 17 00 00 00
# 
name: PHONO
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 14 00 00 00
# 
name: TUNER
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 16 00 00 00
# 
name: TAPE - Record/Pause
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 04 00 00 00
# 
name: TAPE DECK A/B
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 06 00 00 00
# 
name: TAPE RWD
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 01 00 00 00
# 
name: TAPE PLAY
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 00 00 00 00
# 
name: TAPE FFWD
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 02 00 00 00
# 
name: TAPE DIR A
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 07 00 00 00
# 
name: TAPE STOP
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 03 00 00 00
# 
name: TAPE DIR B
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 40 00 00 00
# 
name: CD DISC SKIP
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 4F 00 00 00
# 
name: CD BACK
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 0B 00 00 00
# 
name: CD PLAY
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 08 00 00 00
# 
name: CD FWD
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 0A 00 00 00
# 
name: CD REWIND
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 0D 00 00 00
# 
name: CD STOP/PAUSE
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 09 00 00 00
# 
name: CD FFWD
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 0C 00 00 00
# 
name: TUNER PRESET-
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 11 00 00 00
# 
name: TUNER PRESET+
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 10 00 00 00
# 
name: TUNER A/B/C/D/E
type: parsed
protocol: NEC
address: 7A 00 00 00
command: 12 00 00 00