Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 20 40 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 20 40 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 20 40 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 20 40 00 00
command: 03 00 00 00
#
name: Mem2
type: parsed
protocol: NECext
address: 20 40 00 00
command: 04 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 20 40 00 00
command: 05 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 20 40 00 00
command: 06 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 20 40 00 00
command: 07 00 00 00
#
name: Mem3
type: parsed
protocol: NECext
address: 20 40 00 00
command: 08 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 20 40 00 00
command: 09 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 20 40 00 00
command: 0A 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 20 40 00 00
command: 0B 00 00 00
#
name: Mem4
type: parsed
protocol: NECext
address: 20 40 00 00
command: 0C 00 00 00
#
name: LAST
type: parsed
protocol: NECext
address: 20 40 00 00
command: 0D 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 20 40 00 00
command: 0F 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 20 40 00 00
command: 10 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 20 40 00 00
command: 11 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 20 40 00 00
command: 12 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 20 40 00 00
command: 13 00 00 00
#
name: ChMode
type: parsed
protocol: NECext
address: 20 40 00 00
command: 14 00 00 00
#
name: FMode
type: parsed
protocol: NECext
address: 20 40 00 00
command: 15 00 00 00
#
name: Mem1
type: parsed
protocol: NECext
address: 20 40 00 00
command: 17 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 20 40 00 00
command: 18 00 00 00
#
name: LCR
type: parsed
protocol: NECext
address: 20 40 00 00
command: 19 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 20 40 00 00
command: 1A 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 20 40 00 00
command: 1B 00 00 00
#
name: PCh
type: parsed
protocol: NECext
address: 20 40 00 00
command: 1C 00 00 00
#
name: PLock
type: parsed
protocol: NECext
address: 20 40 00 00
command: 1D 00 00 00
#
name: PGplusminus
type: parsed
protocol: NECext
address: 20 40 00 00
command: 1E 00 00 00
#
name: FAVORITES
type: parsed
protocol: NECext
address: 20 40 00 00
command: 1F 00 00 00
#
name: Fminus
type: parsed
protocol: NECext
address: 20 40 00 00
command: 40 00 00 00
#
name: CFT
type: parsed
protocol: NECext
address: 20 40 00 00
command: 41 00 00 00
#
name: Fplus
type: parsed
protocol: NECext
address: 20 40 00 00
command: 42 00 00 00
#
name: TCCATV
type: parsed
protocol: NECext
address: 20 40 00 00
command: 43 00 00 00
