Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 01 00 00 00
command: 01 00 00 00
#
name: TV/R
type: parsed
protocol: NECext
address: 01 00 00 00
command: 02 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 01 00 00 00
command: 06 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 07 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 08 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 01 00 00 00
command: 0F 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 01 00 00 00
command: 10 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 01 00 00 00
command: 11 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 01 00 00 00
command: 12 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 01 00 00 00
command: 13 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 01 00 00 00
command: 14 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 01 00 00 00
command: 15 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 01 00 00 00
command: 16 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 01 00 00 00
command: 17 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 01 00 00 00
command: 18 00 00 00
#
name: A/B
type: parsed
protocol: NECext
address: 01 00 00 00
command: 24 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 01 00 00 00
command: 27 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 01 00 00 00
command: 2B 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 01 00 00 00
command: 2E 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 01 00 00 00
command: 2F 00 00 00
#
name: ARROW_UP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 32 00 00 00
#
name: ARROW_DOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 33 00 00 00
#
name: ARROW_LEFT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 34 00 00 00
#
name: ARROW_RIGHT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 35 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 01 00 00 00
command: 36 00 00 00
#
name: LIST
type: parsed
protocol: NECext
address: 01 00 00 00
command: 37 00 00 00
