Filetype: IR signals file
Version: 1
#
name: INPUT_SOURCE
type: parsed
protocol: NECext
address: 07 07 00 00
command: 01 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 07 07 00 00
command: 02 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 07 07 00 00
command: 04 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 07 07 00 00
command: 05 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 07 07 00 00
command: 06 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 07 07 00 00
command: 07 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 07 07 00 00
command: 08 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 07 07 00 00
command: 09 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 07 07 00 00
command: 0A 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 07 07 00 00
command: 0B 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 07 07 00 00
command: 0C 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 07 07 00 00
command: 0D 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 07 07 00 00
command: 0E 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 07 07 00 00
command: 0F 00 00 00
#
name: CHANNEL_-
type: parsed
protocol: NECext
address: 07 07 00 00
command: 10 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 07 07 00 00
command: 11 00 00 00
#
name: CHANNEL_+
type: parsed
protocol: NECext
address: 07 07 00 00
command: 12 00 00 00
#
name: LAST
type: parsed
protocol: NECext
address: 07 07 00 00
command: 13 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 07 07 00 00
command: 1A 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 07 07 00 00
command: 1F 00 00 00
#
name: AD/SUBT
type: parsed
protocol: NECext
address: 07 07 00 00
command: 25 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 07 07 00 00
command: 2D 00 00 00
#
name: E-MANUAL
type: parsed
protocol: NECext
address: 07 07 00 00
command: 3F 00 00 00
#
name: TOOLS
type: parsed
protocol: NECext
address: 07 07 00 00
command: 4B 00 00 00
#
name: GUIDE
type: parsed
protocol: NECext
address: 07 07 00 00
command: 4F 00 00 00
#
name: RETURN
type: parsed
protocol: NECext
address: 07 07 00 00
command: 58 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 07 07 00 00
command: 60 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 07 07 00 00
command: 61 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: 07 07 00 00
command: 62 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: 07 07 00 00
command: 65 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 07 07 00 00
command: 68 00 00 00
#
name: CH_LIST
type: parsed
protocol: NECext
address: 07 07 00 00
command: 6B 00 00 00
#
name: SMART_HUB
type: parsed
protocol: NECext
address: 07 07 00 00
command: 79 00 00 00
#
name: 3D
type: parsed
protocol: NECext
address: 07 07 00 00
command: 9F 00 00 00
