Filetype: IR signals file
Version: 1
# 
# Telefunken TV L55U405B4CW , JMB JT0122005B/01, Bush DLED32265HDDVDB
# Remote: RC4875
#
# On JMB/Bush non Smart TV's 
# SMART_HOME will not work.
# 
name: POWER
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0C 00 00 00
# 
name: VOL+
type: parsed
protocol: RC5
address: 01 00 00 00
command: 10 00 00 00
# 
name: VOL-
type: parsed
protocol: RC5
address: 01 00 00 00
command: 11 00 00 00
# 
name: CH+
type: parsed
protocol: RC5
address: 01 00 00 00
command: 20 00 00 00
# 
name: CH-
type: parsed
protocol: RC5
address: 01 00 00 00
command: 21 00 00 00
# 
name: UP
type: parsed
protocol: RC5
address: 01 00 00 00
command: 14 00 00 00
# 
name: DOWN
type: parsed
protocol: RC5
address: 01 00 00 00
command: 13 00 00 00
# 
name: LEFT
type: parsed
protocol: RC5
address: 01 00 00 00
command: 15 00 00 00
# 
name: RIGHT
type: parsed
protocol: RC5
address: 01 00 00 00
command: 16 00 00 00
# 
name: OK
type: parsed
protocol: RC5
address: 01 00 00 00
command: 35 00 00 00
# 
name: BACK
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0A 00 00 00
# 
name: EXIT
type: parsed
protocol: RC5
address: 01 00 00 00
command: 25 00 00 00
# 
name: SMART_HOME
type: parsed
protocol: RC5
address: 01 00 00 00
command: 2E 00 00 00
# 
name: SOURCE
type: parsed
protocol: RC5
address: 01 00 00 00
command: 38 00 00 00
# 
name: MENU
type: parsed
protocol: RC5
address: 01 00 00 00
command: 30 00 00 00
# 
name: Q-MENU
type: parsed
protocol: RC5
address: 01 00 00 00
command: 2B 00 00 00
# 
name: MUTE
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0D 00 00 00
# 
name: 1
type: parsed
protocol: RC5
address: 01 00 00 00
command: 01 00 00 00
# 
name: 2
type: parsed
protocol: RC5
address: 01 00 00 00
command: 02 00 00 00
# 
name: 3
type: parsed
protocol: RC5
address: 01 00 00 00
command: 03 00 00 00
# 
name: 4
type: parsed
protocol: RC5
address: 01 00 00 00
command: 04 00 00 00
# 
name: 5
type: parsed
protocol: RC5
address: 01 00 00 00
command: 05 00 00 00
# 
name: 6
type: parsed
protocol: RC5
address: 01 00 00 00
command: 06 00 00 00
# 
name: 7
type: parsed
protocol: RC5
address: 01 00 00 00
command: 07 00 00 00
# 
name: 8
type: parsed
protocol: RC5
address: 01 00 00 00
command: 08 00 00 00
# 
name: 9
type: parsed
protocol: RC5
address: 01 00 00 00
command: 09 00 00 00
# 
name: 0
type: parsed
protocol: RC5
address: 01 00 00 00
command: 00 00 00 00
# 
name: CH_LIST
type: parsed
protocol: RC5
address: 01 00 00 00
command: 26 00 00 00
# 
name: PREV_CH
type: parsed
protocol: RC5
address: 01 00 00 00
command: 22 00 00 00
# 
name: INFO
type: parsed
protocol: RC5
address: 01 00 00 00
command: 12 00 00 00
# 
name: USB
type: parsed
protocol: RC5
address: 01 00 00 00
command: 39 00 00 00
# 
name: P_GUIDE
type: parsed
protocol: RC5
address: 01 00 00 00
command: 2F 00 00 00
# 
name: 1ST_CH
type: parsed
protocol: RC5
address: 01 00 00 00
command: 3B 00 00 00
# 
name: CH_NET_TYPE
type: parsed
protocol: RC5
address: 01 00 00 00
command: 1A 00 00 00
# 
name: LANG
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0F 00 00 00
# 
name: SUBTITLE
type: parsed
protocol: RC5
address: 01 00 00 00
command: 1F 00 00 00
# 
name: ASPECT
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0B 00 00 00
# 
name: REWIND
type: parsed
protocol: RC5
address: 01 00 00 00
command: 1B 00 00 00
# 
name: PAUSE
type: parsed
protocol: RC5
address: 01 00 00 00
command: 31 00 00 00
# 
name: PLAY
type: parsed
protocol: RC5
address: 01 00 00 00
command: 19 00 00 00
# 
name: F_FORWARD
type: parsed
protocol: RC5
address: 01 00 00 00
command: 1C 00 00 00
# 
name: STOP
type: parsed
protocol: RC5
address: 01 00 00 00
command: 18 00 00 00
# 
name: RECORD
type: parsed
protocol: RC5
address: 01 00 00 00
command: 33 00 00 00
# 
name: RED
type: parsed
protocol: RC5
address: 01 00 00 00
command: 37 00 00 00
# 
name: GREEN
type: parsed
protocol: RC5
address: 01 00 00 00
command: 36 00 00 00
# 
name: YELLOW
type: parsed
protocol: RC5
address: 01 00 00 00
command: 32 00 00 00
# 
name: BLUE
type: parsed
protocol: RC5
address: 01 00 00 00
command: 34 00 00 00
