Filetype: IR signals file
Version: 1
#
# Sony Bravia KD-55XF80xx, KD-49XF80xx, KD-43XF80xx.ir
#
name: POWER
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 15 00 00 00
# 
name: Input
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 25 00 00 00
# 
name: Home
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 60 00 00 00
# 
name: Apps
type: parsed
protocol: SIRC15
address: C4 00 00 00
command: 2A 00 00 00
# 
name: Tv
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 24 00 00 00
# 
name: Left
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 34 00 00 00
# 
name: Right
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 33 00 00 00
# 
name: Up
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 74 00 00 00
# 
name: Down
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 75 00 00 00
# 
name: Enter
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 65 00 00 00
#
name: Back
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 23 00 00 00
# 
name: MUTE
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 14 00 00 00
# 
name: VOL+
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 12 00 00 00
# 
name: VOL-
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 13 00 00 00
# 
name: CH+
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 10 00 00 00
#
name: CH-
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 11 00 00 00
# 
name: Play
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 1A 00 00 00
# 
name: Pause
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 19 00 00 00
# 
name: Stop
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 18 00 00 00
# 
name: Fwd
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 1C 00 00 00
# 
name: Rew
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 1B 00 00 00
# 
name: Prev
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 3C 00 00 00
# 
name: Next
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 3D 00 00 00
# 
name: Rec
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 20 00 00 00
# 
name: Netflix
type: parsed
protocol: SIRC15
address: 1A 00 00 00
command: 7C 00 00 00
# 
name: Google_play
type: parsed
protocol: SIRC15
address: C4 00 00 00
command: 46 00 00 00
# 
name: Red
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 25 00 00 00
# 
name: Green
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 26 00 00 00
# 
name: Yellow
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 27 00 00 00
# 
name: Blue
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 24 00 00 00
# 
name: Action_menu
type: parsed
protocol: SIRC15
address: C4 00 00 00
command: 4B 00 00 00
# 
name: Guide
type: parsed
protocol: SIRC15
address: A4 00 00 00
command: 5B 00 00 00
# 
name: Help
type: parsed
protocol: SIRC15
address: C4 00 00 00
command: 4D 00 00 00
# 
name: Title_list
type: parsed
protocol: SIRC15
address: 1A 00 00 00
command: 65 00 00 00
# 
name: Audio
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 17 00 00 00
# 
name: Screen___
type: parsed
protocol: SIRC15
address: 97 00 00 00
command: 28 00 00 00
# 
name: Swap
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 3B 00 00 00
# 
name: Dig_analo
type: parsed
protocol: SIRC15
address: 77 00 00 00
command: 0D 00 00 00
# 
name: Tv_radio
type: parsed
protocol: SIRC15
address: 1A 00 00 00
command: 57 00 00 00
# 
name: Exit
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 63 00 00 00
# 
name: Ext_box_menu
type: parsed
protocol: SIRC15
address: C4 00 00 00
command: 49 00 00 00
# 
name: 1
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 00 00 00 00
# 
name: 2
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 01 00 00 00
# 
name: 3
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 02 00 00 00
# 
name: 4
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 03 00 00 00
# 
name: 5
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 04 00 00 00
# 
name: 6
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 05 00 00 00
# 
name: 7
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 06 00 00 00
# 
name: 8
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 07 00 00 00
# 
name: 9
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 08 00 00 00
# 
name: 0
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 09 00 00 00
# 
name: I_plus
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 3A 00 00 00
# 
name: Txt
type: parsed
protocol: SIRC
address: 01 00 00 00
command: 3F 00 00 00
